#lighthack Demo Station

Does it look like these TouchOSC configurations are missing something? Good. Check out these //TODO activities.

# Console Prerequisite:

* Patch channel 1 thru 5 as a SolaFrame Theatre fixture

Box 1.ino

//TODO: Possible activities

* Update the version number to v2.0.0.0
* Change “waiting for eos” to “Hello World!”
* Change the keys from Next and Last to Full and Out
* Change the encoder sensitivity (PAN\_SCALE and TILT\_SCALE)
* Change the Pan and Tilt encoders to Intensity and Shutter\_Strobe
  + Be aware there are multiple places to update
  + Eos calls Intensity “Intens” and shutter strobe “Shutter\_Strobe”

Have an idea? Try it out!