Touch OSC Demo Station

Does it look like these TouchOSC configurations are missing something? Good. Check out these //TODO activities.

Demo

//TODO: Possible activities

* Make numbers 0, 2 < 9, and the Thru button work on the number pad
* Map the second yellow fader to Fader ½
* Make the back button work
* Try to make the command line follow user 2
* Set your own command on the ??? button
* Add another row of buttons – perhaps FL, Out, and Level?

Demo\_Encoders

//TODO: Possible activities

* Check out the difference between the Intens encoder and the Cyan encoder
  + Hint: Watch when you select channel 1 how the encoders react
* Make Magenta and Yellow work like Cyan
* Change the CMY encoders to be dynamic encoders like Intensity
* Play with Pan/Tilt
* Try changing the Pan/Tilt to a CIE xy color control
  + Hint: Search the manual for “xy”

Have an idea? Try it out!